**Some MUST READ tips before you do the upgrade**

1. Software V2.0.5 MUST WORK WITH firmware V3.0.6

2. Clear all the previous settings of GD-77 before upgrade, and it is suggested to backup all the beta you need

3. After successfully upgraded, the CSV file from old version V1.X.X will NOT be compatible with the completely new version V2.X.X. You will have to use the new CPS to import a new template to do the bulk operation;

4. Please do follow the rules that mentioned above, and if you failed to upgrade your radio please reset it all and try again.

**What’s NEW with this software & firmware**

**1. ADD VFO**

How to enter VFO mode: short press the right arrow key on the keypad → to switch the VFO and MR; short press the left arrow key ← to switch the frequency bands.



**2. Contact ID**

The number of digital contact IDs has been expanded from 256 to 1000.



**3. Scan list & Channel list**

The number of scan list is expanded from 16 to 64, and the number of channel list is expanded from 16 to 31.



**4. DMR ID Database**

We provide a total of 49607 people with DMR IDs registered globally, under the file name “datadump”. As GD-77 can only support saving the top 10000 from the list as default, please select the IDs you want to add.

For more details of the import operation, see: DMR ID operation.

Note:

1：Read and write DMR ID data: Press **SK2**+**Menu**+**# key** at the same time to turn on radio

2：Please DO NOT delete or modify the first row



5. Fix the bug of zones lost

6. Fix the bug of distorted audio